Text

Description automatically generated with medium confidence

* Alpha and Beta values are set based upon the precision of the Radar
  + Alpha and Beta values near 1 are used in systems with high precision
  + For systems with low precision the values are set closer to 0
  + A system where the alpha and/or beta values are set 0 is an example where the measurement has no bearing on the estimate